How to install Raid 5:

1-go to the disk management und right click of the disk not online then make it online.

2-then go to again and right click and choose intimidation. Then choos all disks und GPT option.

3-then right click und select convert to dynamic disk and select all disks.

4-right click and select new volume raid 5—select all disks-one letter then quick scan

Configuration swtch:always go to config t

1-hostname arbion

2-enable password then give it

3-show vlan to show allEthernet

4-to create vlan :vlan 10 then give it name –name It

5-to give ethernet:interface fastethernet 0/1 ----switchport access mode---switchport access vlan10

6-to give more than one :interface range festethernet 0/2-10—then the same

7- if you want to show in config mode:do show vlan

8-to give ip address for vlan –interface vlan 10—ip address 10.10.10.0 255.255.255.0

9-to show t hip—show ip interface brief

10-ip routing